Open topic with navigation

You are here: Publish Results > About > Haulage Results > Haulage Results Export
GEOVIA MineSched

|  | Print

# Export Haulage Results

The Export haulage results button opens the Export Haulage Results form, which you use to select the product, file format, and location to which you want to save the haulage results. The coordinates of the points of the haulage routes are saved to all file formats. If the file format you select supports additional attributes, values for each of the following are also output to the results file for each haulage route:

- name of the source location
- period number
- number of the source block
- number of the source group
- name of the destination
- number of the destination block
- name of the material class
- volume
- mass
- name of the haulage route
- velocity

Note: If you save to a GEOVIA Surpac string file, all attributes are written to the first point of each segment. Only the velocity is written to the D1 fields of all other points in each segment. The reason that only one velocity value is written to each point is because each string now includes points for the full and empty path. In comparison, in MineSched 8.0 and earlier the haulage strings contained only one set of points that represented both the full and empty paths, and each point was assigned two velocities: one for the full velocity in the D10 field and one for the empty velocity in the D11 field.

If you choose to save the haulage results to a GEOVIA GEMS project, the Output Format field is replaced by the Workspace Name field. You use the Ellipsis button, to the right of the Workspace Name field, to browse for the project to which you want to save the haulage results. After you select the GEMS project, the Workspace Browser form appears, in which you select the workspace to which you want to export the haulage results. Finally, you use the Ellipsis button to the right of the Field Mapping field to open the Field Mappings form. In the Field Mappings form, you select the subtable of the workspace to which the results are exported, and map the haulage attributes to the fields of the subtable to define the fields to which the attributes are exported.

### Fields of the Export Haulage Results Form

Field | Description
--- | ---
Product | The product in which you want to be able to open the exported haulage results. Options are: Surpac GEMS Minex AutoCAD Datamine MapInfo Micromine Microstation Vulcan
Output Format | The file format to which you want to save the haulage results. The list of file formats available is controlled by the Product selected.
File Path | The location to which you want to save the haulage results, and the file name you want to use for the exported results file.
Workspace Name | The name of the GEMS project and workspace within the project to which you want to export the haulage results. To select the project and workspace, click the Ellipsis button.
Field Mapping | The fields of the GEMS workspace to which you want to export the haulage results. To map the fields, click the Ellipsis button.

### See also

- Haulage
- Haulage Results

Open topic with navigation