             BLAST HOLE DESIGN - LOAD BLAST HOLES TO DATABASE REPORTMar 01, 2011




Load commencing on 01-Mar-11
Loading collar table - collar
Loading survey table - survey
Loading charging table - 
Loading sample table - sample
=====================================================================

Ignoring hole depth from             5.00 to             7.20 after sample (721(BP1)-1)
Ignoring hole depth from             5.00 to             7.20 after sample (722(BP1)-2)
Ignoring hole depth from             5.00 to             7.20 after sample (766(BP1)-3)
Ignoring hole depth from             5.00 to             7.20 after sample (767(BP1)-4)
Ignoring hole depth from             5.00 to             7.20 after sample (768(BP1)-5)
Ignoring hole depth from             5.00 to             7.20 after sample (769(BP1)-6)
Ignoring hole depth from             5.00 to             7.20 after sample (770(BP1)-7)
Ignoring hole depth from             5.00 to             7.20 after sample (771(BP1)-8)
Ignoring hole depth from             5.00 to             7.20 after sample (772(BP1)-9)
Ignoring hole depth from             5.00 to             7.20 after sample (773(BP1)-10)
Ignoring hole depth from             5.00 to             7.20 after sample (774(BP1)-11)
Ignoring hole depth from             5.00 to             7.20 after sample (775(BP1)-12)
Ignoring hole depth from             5.00 to             7.20 after sample (776(BP1)-13)
Ignoring hole depth from             5.00 to             7.20 after sample (777(BP1)-14)
Ignoring hole depth from             5.00 to             7.20 after sample (778(BP1)-15)
Ignoring hole depth from             5.00 to             7.20 after sample (779(BP1)-16)
Ignoring hole depth from             5.00 to             7.20 after sample (780(BP1)-17)
Ignoring hole depth from             5.00 to             7.20 after sample (781(BP1)-18)
Ignoring hole depth from             5.00 to             7.20 after sample (782(BP1)-19)
Ignoring hole depth from             5.00 to             7.20 after sample (783(BP1)-20)
Ignoring hole depth from             5.00 to             7.20 after sample (784(BP1)-21)
Ignoring hole depth from             5.00 to             7.20 after sample (811(BP1)-22)
Ignoring hole depth from             5.00 to             7.20 after sample (812(BP1)-23)
Ignoring hole depth from             5.00 to             7.20 after sample (813(BP1)-24)
Ignoring hole depth from             5.00 to             7.20 after sample (814(BP1)-25)
Ignoring hole depth from             5.00 to             7.20 after sample (815(BP1)-26)
Ignoring hole depth from             5.00 to             7.20 after sample (816(BP1)-27)
Ignoring hole depth from             5.00 to             7.20 after sample (817(BP1)-28)
Ignoring hole depth from             5.00 to             7.20 after sample (818(BP1)-29)
Ignoring hole depth from             5.00 to             7.20 after sample (819(BP1)-30)
Ignoring hole depth from             5.00 to             7.20 after sample (820(BP1)-31)
Ignoring hole depth from             5.00 to             7.20 after sample (821(BP1)-32)
Ignoring hole depth from             5.00 to             7.20 after sample (822(BP1)-33)
Ignoring hole depth from             5.00 to             7.20 after sample (823(BP1)-34)
Ignoring hole depth from             5.00 to             7.20 after sample (824(BP1)-35)
Ignoring hole depth from             5.00 to             7.20 after sample (825(BP1)-36)
Ignoring hole depth from             5.00 to             7.20 after sample (826(BP1)-37)
Ignoring hole depth from             5.00 to             7.20 after sample (827(BP1)-38)
Ignoring hole depth from             5.00 to             7.20 after sample (828(BP1)-39)
Ignoring hole depth from             5.00 to             7.20 after sample (829(BP1)-40)
Ignoring hole depth from             5.00 to             7.20 after sample (830(BP1)-41)
Ignoring hole depth from             5.00 to             7.20 after sample (855(BP1)-42)
Ignoring hole depth from             5.00 to             7.20 after sample (856(BP1)-43)
Ignoring hole depth from             5.00 to             7.20 after sample (857(BP1)-44)
Ignoring hole depth from             5.00 to             7.20 after sample (858(BP1)-45)
Ignoring hole depth from             5.00 to             7.20 after sample (859(BP1)-46)
Ignoring hole depth from             5.00 to             7.20 after sample (860(BP1)-47)
Ignoring hole depth from             5.00 to             7.20 after sample (861(BP1)-48)
Ignoring hole depth from             5.00 to             7.20 after sample (862(BP1)-49)
Ignoring hole depth from             5.00 to             7.20 after sample (863(BP1)-50)
Ignoring hole depth from             5.00 to             7.20 after sample (864(BP1)-51)
Ignoring hole depth from             5.00 to             7.20 after sample (865(BP1)-52)
Ignoring hole depth from             5.00 to             7.20 after sample (866(BP1)-53)
Ignoring hole depth from             5.00 to             7.20 after sample (867(BP1)-54)
Ignoring hole depth from             5.00 to             7.20 after sample (868(BP1)-55)
Ignoring hole depth from             5.00 to             7.20 after sample (869(BP1)-56)
Ignoring hole depth from             5.00 to             7.20 after sample (870(BP1)-57)
Ignoring hole depth from             5.00 to             7.20 after sample (871(BP1)-58)
Ignoring hole depth from             5.00 to             7.20 after sample (872(BP1)-59)
Ignoring hole depth from             5.00 to             7.20 after sample (873(BP1)-60)
Ignoring hole depth from             5.00 to             7.20 after sample (874(BP1)-61)
Ignoring hole depth from             5.00 to             7.20 after sample (875(BP1)-62)
Ignoring hole depth from             5.00 to             7.20 after sample (900(BP1)-63)
Ignoring hole depth from             5.00 to             7.20 after sample (901(BP1)-64)
Ignoring hole depth from             5.00 to             7.20 after sample (902(BP1)-65)
Ignoring hole depth from             5.00 to             7.20 after sample (903(BP1)-66)
Ignoring hole depth from             5.00 to             7.20 after sample (904(BP1)-67)
Ignoring hole depth from             5.00 to             7.20 after sample (905(BP1)-68)
Ignoring hole depth from             5.00 to             7.20 after sample (906(BP1)-69)
Ignoring hole depth from             5.00 to             7.20 after sample (907(BP1)-70)
Ignoring hole depth from             5.00 to             7.20 after sample (908(BP1)-71)
Ignoring hole depth from             5.00 to             7.20 after sample (909(BP1)-72)
Ignoring hole depth from             5.00 to             7.20 after sample (910(BP1)-73)
Ignoring hole depth from             5.00 to             7.20 after sample (911(BP1)-74)
Ignoring hole depth from             5.00 to             7.20 after sample (912(BP1)-75)
Ignoring hole depth from             5.00 to             7.20 after sample (913(BP1)-76)
Ignoring hole depth from             5.00 to             7.20 after sample (914(BP1)-77)
Ignoring hole depth from             5.00 to             7.20 after sample (915(BP1)-78)
Ignoring hole depth from             5.00 to             7.20 after sample (916(BP1)-79)
Ignoring hole depth from             5.00 to             7.20 after sample (917(BP1)-80)
Ignoring hole depth from             5.00 to             7.20 after sample (918(BP1)-81)
Ignoring hole depth from             5.00 to             7.20 after sample (919(BP1)-82)
Ignoring hole depth from             5.00 to             7.20 after sample (920(BP1)-83)
Ignoring hole depth from             5.00 to             7.20 after sample (921(BP1)-84)
Ignoring hole depth from             5.00 to             7.20 after sample (945(BP1)-85)
Ignoring hole depth from             5.00 to             7.20 after sample (946(BP1)-86)
Ignoring hole depth from             5.00 to             7.20 after sample (947(BP1)-87)
Ignoring hole depth from             5.00 to             7.20 after sample (948(BP1)-88)
Ignoring hole depth from             5.00 to             7.20 after sample (949(BP1)-89)
Ignoring hole depth from             5.00 to             7.20 after sample (950(BP1)-90)
Ignoring hole depth from             5.00 to             7.20 after sample (951(BP1)-91)
Ignoring hole depth from             5.00 to             7.20 after sample (952(BP1)-92)
Ignoring hole depth from             5.00 to             7.20 after sample (953(BP1)-93)
Ignoring hole depth from             5.00 to             7.20 after sample (954(BP1)-94)
Ignoring hole depth from             5.00 to             7.20 after sample (955(BP1)-95)
Ignoring hole depth from             5.00 to             7.20 after sample (956(BP1)-96)
Ignoring hole depth from             5.00 to             7.20 after sample (957(BP1)-97)
Ignoring hole depth from             5.00 to             7.20 after sample (958(BP1)-98)
Ignoring hole depth from             5.00 to             7.20 after sample (959(BP1)-99)
Ignoring hole depth from             5.00 to             7.20 after sample (960(BP1)-100)
Ignoring hole depth from             5.00 to             7.20 after sample (961(BP1)-101)
Ignoring hole depth from             5.00 to             7.20 after sample (962(BP1)-102)
Ignoring hole depth from             5.00 to             7.20 after sample (963(BP1)-103)
Ignoring hole depth from             5.00 to             7.20 after sample (964(BP1)-104)
Ignoring hole depth from             5.00 to             7.20 after sample (965(BP1)-105)
Ignoring hole depth from             5.00 to             7.20 after sample (966(BP1)-106)
Ignoring hole depth from             5.00 to             7.20 after sample (967(BP1)-107)
Ignoring hole depth from             5.00 to             7.20 after sample (990(BP1)-108)
Ignoring hole depth from             5.00 to             7.20 after sample (991(BP1)-109)
Ignoring hole depth from             5.00 to             7.20 after sample (992(BP1)-110)
Ignoring hole depth from             5.00 to             7.20 after sample (993(BP1)-111)
Ignoring hole depth from             5.00 to             7.20 after sample (994(BP1)-112)
Ignoring hole depth from             5.00 to             7.20 after sample (995(BP1)-113)
Ignoring hole depth from             5.00 to             7.20 after sample (996(BP1)-114)
Ignoring hole depth from             5.00 to             7.20 after sample (997(BP1)-115)
Ignoring hole depth from             5.00 to             7.20 after sample (998(BP1)-116)
Ignoring hole depth from             5.00 to             7.20 after sample (999(BP1)-117)
Ignoring hole depth from             5.00 to             7.20 after sample (1000(BP1)-118)
Ignoring hole depth from             5.00 to             7.20 after sample (1001(BP1)-119)
Ignoring hole depth from             5.00 to             7.20 after sample (1002(BP1)-120)
Ignoring hole depth from             5.00 to             7.20 after sample (1003(BP1)-121)
Ignoring hole depth from             5.00 to             7.20 after sample (1004(BP1)-122)
Ignoring hole depth from             5.00 to             7.20 after sample (1005(BP1)-123)
Ignoring hole depth from             5.00 to             7.20 after sample (1006(BP1)-124)
Ignoring hole depth from             5.00 to             7.20 after sample (1007(BP1)-125)
Ignoring hole depth from             5.00 to             7.20 after sample (1008(BP1)-126)
Ignoring hole depth from             5.00 to             7.20 after sample (1009(BP1)-127)
Ignoring hole depth from             5.00 to             7.20 after sample (1010(BP1)-128)
Ignoring hole depth from             5.00 to             7.20 after sample (1011(BP1)-129)
Ignoring hole depth from             5.00 to             7.20 after sample (1012(BP1)-130)
Ignoring hole depth from             5.00 to             7.20 after sample (1035(BP1)-131)
Ignoring hole depth from             5.00 to             7.20 after sample (1036(BP1)-132)
Ignoring hole depth from             5.00 to             7.20 after sample (1037(BP1)-133)
Ignoring hole depth from             5.00 to             7.20 after sample (1038(BP1)-134)
Ignoring hole depth from             5.00 to             7.20 after sample (1039(BP1)-135)
Ignoring hole depth from             5.00 to             7.20 after sample (1040(BP1)-136)
Ignoring hole depth from             5.00 to             7.20 after sample (1041(BP1)-137)
Ignoring hole depth from             5.00 to             7.20 after sample (1042(BP1)-138)
Ignoring hole depth from             5.00 to             7.20 after sample (1043(BP1)-139)
Ignoring hole depth from             5.00 to             7.20 after sample (1044(BP1)-140)
Ignoring hole depth from             5.00 to             7.20 after sample (1045(BP1)-141)
Ignoring hole depth from             5.00 to             7.20 after sample (1046(BP1)-142)
Ignoring hole depth from             5.00 to             7.20 after sample (1047(BP1)-143)
Ignoring hole depth from             5.00 to             7.20 after sample (1048(BP1)-144)
Ignoring hole depth from             5.00 to             7.20 after sample (1049(BP1)-145)
Ignoring hole depth from             5.00 to             7.20 after sample (1050(BP1)-146)
Ignoring hole depth from             5.00 to             7.20 after sample (1051(BP1)-147)
Ignoring hole depth from             5.00 to             7.20 after sample (1052(BP1)-148)
Ignoring hole depth from             5.00 to             7.20 after sample (1053(BP1)-149)
Ignoring hole depth from             5.00 to             7.20 after sample (1054(BP1)-150)
Ignoring hole depth from             5.00 to             7.20 after sample (1055(BP1)-151)
Ignoring hole depth from             5.00 to             7.20 after sample (1056(BP1)-152)
Ignoring hole depth from             5.00 to             7.20 after sample (1080(BP1)-153)
Ignoring hole depth from             5.00 to             7.20 after sample (1081(BP1)-154)
Ignoring hole depth from             5.00 to             7.20 after sample (1082(BP1)-155)
Ignoring hole depth from             5.00 to             7.20 after sample (1083(BP1)-156)
Ignoring hole depth from             5.00 to             7.20 after sample (1084(BP1)-157)
Ignoring hole depth from             5.00 to             7.20 after sample (1085(BP1)-158)
Ignoring hole depth from             5.00 to             7.20 after sample (1086(BP1)-159)
Ignoring hole depth from             5.00 to             7.20 after sample (1087(BP1)-160)
Ignoring hole depth from             5.00 to             7.20 after sample (1088(BP1)-161)
Ignoring hole depth from             5.00 to             7.20 after sample (1089(BP1)-162)
Ignoring hole depth from             5.00 to             7.20 after sample (1090(BP1)-163)
Ignoring hole depth from             5.00 to             7.20 after sample (1091(BP1)-164)
Ignoring hole depth from             5.00 to             7.20 after sample (1092(BP1)-165)
Ignoring hole depth from             5.00 to             7.20 after sample (1093(BP1)-166)
Ignoring hole depth from             5.00 to             7.20 after sample (1094(BP1)-167)
Ignoring hole depth from             5.00 to             7.20 after sample (1095(BP1)-168)
Ignoring hole depth from             5.00 to             7.20 after sample (1096(BP1)-169)
Ignoring hole depth from             5.00 to             7.20 after sample (1097(BP1)-170)
Ignoring hole depth from             5.00 to             7.20 after sample (1098(BP1)-171)
Ignoring hole depth from             5.00 to             7.20 after sample (1099(BP1)-172)
Ignoring hole depth from             5.00 to             7.20 after sample (1100(BP1)-173)
Ignoring hole depth from             5.00 to             7.20 after sample (1125(BP1)-174)
Ignoring hole depth from             5.00 to             7.20 after sample (1126(BP1)-175)
Ignoring hole depth from             5.00 to             7.20 after sample (1127(BP1)-176)
Ignoring hole depth from             5.00 to             7.20 after sample (1128(BP1)-177)
Ignoring hole depth from             5.00 to             7.20 after sample (1129(BP1)-178)
Ignoring hole depth from             5.00 to             7.20 after sample (1130(BP1)-179)
Ignoring hole depth from             5.00 to             7.20 after sample (1131(BP1)-180)
Ignoring hole depth from             5.00 to             7.20 after sample (1132(BP1)-181)
Ignoring hole depth from             5.00 to             7.20 after sample (1133(BP1)-182)
Ignoring hole depth from             5.00 to             7.20 after sample (1134(BP1)-183)
Ignoring hole depth from             5.00 to             7.20 after sample (1135(BP1)-184)
Ignoring hole depth from             5.00 to             7.20 after sample (1136(BP1)-185)
Ignoring hole depth from             5.00 to             7.20 after sample (1137(BP1)-186)
Ignoring hole depth from             5.00 to             7.20 after sample (1138(BP1)-187)
Ignoring hole depth from             5.00 to             7.20 after sample (1139(BP1)-188)
Ignoring hole depth from             5.00 to             7.20 after sample (1140(BP1)-189)
Ignoring hole depth from             5.00 to             7.20 after sample (1141(BP1)-190)
Ignoring hole depth from             5.00 to             7.20 after sample (1142(BP1)-191)
Ignoring hole depth from             5.00 to             7.20 after sample (1143(BP1)-192)
Ignoring hole depth from             5.00 to             7.20 after sample (1144(BP1)-193)

=====================================================================

End of Load blast holes to database report
                                                                     Page 1 of 1
