Open topic with navigation

You are here: Setup Schedule > How to > Define Overall Production Location Constraints
GEOVIA MineSched

|  | Print

# Define Overall Location Constraints

1. In the Location constraints data grid, click Insert.

A new row is added to the data grid.

2. Click the Headings column and select the headings to which you want the constraint to apply.
3. Click the Locations column and select the locations to which you want the constraint to apply.
4. Click the Materials column and select the material classes to which you want the constraint to apply.
5. Click the Unit column and select the unit in which the rate is measured.
6. Click the Value column and type the value for the rate to which the location is constrained.
7. Click the Date/event column and select the date or event on which the constraint is applied to the location.
8. Click the Delay column and type a value for the number of days that must elapse, after the date or event selected, before the constraint is applied to the location.

### See also

- Location Constraints
- Production Rates
- Resource Capacities
- Create a Resource
- Assign a Resource to a Location
- Specify a Resource Capacity
- Specify Additional Production Rate Parameters

Open topic with navigation