Open topic with navigation

You are here: Setup Schedule > About > Parameters > Polygon Precedences
GEOVIA MineSched

|  | Print

# Polygon Precedences

You use the Polygon precedences data grid to define polygon precedences between locations.

If polygon precedences exist between two locations, mining in a polygon or a solid in the secondary location cannot start until mining of the same numbered polygon or solid in the primary location is completed.

You can define the polygon precedences in the Polygon precedences data grid, or you can use the spreadsheet view. To access the spreadsheet view, select Spreadsheet > Enable Spreadsheet Views, and then select the Polygon Precedences spreadsheet. When the Polygon Precedences spreadsheet is enabled, it replaces the Polygon precedences data grid in the Parameters tab.

### Columns in the Polygon Precedences Data Grid

Column | Description
--- | ---
Primary | The location in which the polygon or solid must be mined before the polygon or solid of the same number can be mined in the Secondary location.
Secondary | The location that cannot be mined until the polygon or solid of the same number is mined in the Primary location.

### See also

- Precedences
- Production Parameters
- Precedences Parameters
- Spatial Relationships
- Manual Precedences
- Locations

Open topic with navigation