Open topic with navigation

You are here: Setup Schedule > About > Material Flow > Haulage > Haulage Routes
GEOVIA MineSched

|  | Print

# Haulage Routes

You use the Haulage routes tab to define the haulage routes that you assign to material movement rules in the Material movement data grid.

The Haulage tab contains the Haulage routes data grid and the Full path, Empty path, and Bench tabs. You use the Haulage routes tab to create the haulage routes, associate a truck type with each haulage route, and define the haulage paths that make up each haulage route. Within the Full path, Empty path, and Bench tabs, you use the:

- Segments data grid to define the:
  - full path
  - empty path
  - bench haulage paths
- Velocities data grid to assign velocities to either:
  - segments of the haulage paths
  - individual points within the segments

### Columns in the Haulage Routes Data Grid

Column | Description
--- | ---
Route name | The name of the haulage route. You use the name in the Haulage field of the Material movement data grid to assign the route to the material movement. Note: If any parameters are not defined, or not correct for a haulage route, a warning icon is displayed next to the Route name.
Truck | The truck that transports material on the haulage route.

### See also

- Full path
- Empty path
- Bench
- Truck Types
- Material Movement

Open topic with navigation