                             Blast work order report                Mar 01, 2011




Detailed report
Blast pattern : BP1
Rock mass classification : Laterite

Prepared by : Tutorial
Product requirement : Immediate
Blasting notes : Blast Today 5-00pm

Particulars                                   Value                      
-----------------------------------------------------------------------
Date                                          01-Mar-11                  
Calculation method                            Without using block model  
Collar Elevation(Meter)                       960.000                    
No. of holes in the blast                     830                        
Detonator:Nonel LP-DET 2 (400.00ms)           830                        
Total no. of detonators                       830                        
Blasting method                               row by row                 
ANFO 0.8(Kilogram)                            29725.75                   
Anzomex G (PG)(Number of booster cartridges)  830.00                     
Total mass of the explosive(Kilogram)         29817.05                   
Explosive mass per unit hole length           6.30                       
Blasted volume(Cubic meter)                   38156.93                   
Blasted mass(Kilogram)                        83945238.97                

**** Surface delays are not included in this report.  Please calculate required surface delays manually ****
                                                                     Page 1 of 1
